1. (Single) In which view is the *sysname Huawei* command used to set the device name to Huawei?( B )
2. User view
3. System view
4. interface view
5. protocol view
6. (Single) Which of the following statements about storage devices is false?( B )
7. Flash is a non-volatile memory. Data will not be lost after a power failure.
8. NVRAM non-volatile random access memory for configuration files
9. The SD card can store system files, configuration files, and logs.
10. SDRAM is equivalent to the memory of a computer.
11. (Multiple) Which of the following views cannot be used by the save command?( BCD )
12. User view
13. System view
14. Interface view
15. Protocol view
16. (True or False) Huawei VRP does not have a file system. Therefore, you cannot perform operations on files. You must use external tools to perform operations on files.( B )
17. True
18. False
19. (True or False) When using the console port to manage the device, only one person can perform this operation at the same time. When using the VTY port, multiple persons can perform this operation at the same time.( A )
20. True
21. False
22. What is the VRP version currently used by Huawei datacom devices?

A: Currently, most Huawei datacom products use VRPv5, and a few products such as NE series routers use VRPv8.

1. What is the maximum number of users that are allowed to log in to a Huawei device through the console port concurrently?

A: A Huawei device allows only one user to log in through the console interface at a time. Therefore, the console user ID is fixed at 0.

1. How do I specify the configuration file for next startup if a device has multiple configuration files?

A: To specify a configuration file for next startup, run the **startup saved-configuration** [ *configuration-file* ] command. The value of *configuration-file* should contain both the file name and extension.