1. (Single) Which of the following operations is used by the managed device to report alarms in SNMPv1?( C )
2. Get
3. Set
4. Inform
5. Trap
6. (Single) On an SNMP-based network, what is used to indicate information that can be queried and set by the agent process? ( A )
7. NMS
8. Agent process
9. MIB
10. Managed devices
11. (Multiple) Which of the following are key capabilities of NCE?( ABCD )
12. Full-lifecycle automation
13. Intelligent closed-loop based on big data and AI
14. Open Programmable Enables Scenario-based App Ecosystem
15. Large-capacity full-cloud platform
16. (True or false) SNMPv3 has the same working mechanism as SNMPv1 and SNMPv2c, but adds header data and security parameters.( A )
17. True
18. False
19. (True or false) YANG is a data modeling language that standardizes NETCONF data content.( A )
20. True
21. False
22. (Single) In SNMPv1, which of the following operations is used by a managed device to report traps? ( C )
23. Get-Request
24. Set-Request
25. Trap
26. Response