1. (Single) Which one of the following rules is a valid basic ACL rule? ( C )
2. rule permit ip
3. rule deny ip
4. rule permit source any
5. rule deny tcp source any
6. (Single) Which of the following ACL rules can the traffic destined for 192.168.1.1/24 be permitted?( A )
7. rule permit source 192.168.1.1 0.0.0.255
8. rule permit source 192.168.1.0 0.0.0.254
9. rule permit source 192.168.0.0 0.0.0.255
10. rule deny source any
11. (Single) Which of the following cannot be controlled by ACL 3001?( D )
12. Destination address
13. Source address
14. Destination port number
15. Packet length
16. (Multiple) What are the applications of ACLs?( ABCD )
17. Provide means of controlling communication traffic
18. Is a basic means of providing network security access.
19. Called in QoS
20. Matches routes.
21. (True or False) The default step for configuring an ACL is 5. The step can be changed.( A )
22. True
23. False
24. (True or False) The configuration commands of ACL 2001 are as follows:

Rule 5 permit source 192.168.1.1 0.0.0.0

Rule 10 deny source 192.168.1.1 0.0.0.0

Then, the traffic with the destination address 192.168.1.1 is permitted.( A )

1. True
2. False
3. Q:Which parameters can you use to define advanced ACL rules?  
   A:parameters such as the source/destination IP address, source/destination port number, protocol type, and TCP flag (SYN, ACK, or FIN).